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Important Safety Guide

1. Read this README thoroughly before you attempt to install or operate PenMount touch screen.

2. Keep this CD-Rom for later use.

3. Never use sharp material to touch or write on the touch screen.

4. Using finger or the providing PenMount pen to touch or write on the touch screen, never use pen with ink or pencil on this touch screen.

Contact your supplier for clarification on any part of this CD-ROM.

PENMOUNT TOUCH SCREEN Kits introudction

 PenMount Touch Screen Kits is a turnkey solution to upgrade your product to have touch function. PenMount Touch Screen Kits include three items:

a. Touch screen

b. PenMount Controller board or ASIC

c. CD-ROM for PenMount Driver diskettes

 PenMount touch screen is resistive type touch screen. There are two designs: 4-wire and 8-wire touch screens. For diagonal size larger than 8”, 8-wire touch screen is provided. And for diagonal size smaller than 7”, we provide 4-wire technology on touch screen.  From the touch screen connector side, 8-pin connector or 4-pin connector, user can easily identify which touch screen is used in your product.

 To assemble the touch screen into the system, the surrounding circuit (silver bus) has to be covered by front bezel of product entirely, and leave the tail side connected to the 4-pin or 8-pin touch screen cable on PenMount touch screen control board.

 There are two types of PenMount touch screen control board for RS-232 interface. Identical function on all boards in different physical dimensions offers a convenience for design-in jobs. The main controller on board is PenMount 9512 series or PenMount 9000 series.  Three cables connect the board to computer and touch screen. The 2-wire power line is for 5V to 12V DC power connection.   The 9-pin cable with D-sub connector should be connected to serial port of the computer. And the 4-wire or 8-wire cable is connected to the touch screen

.

 PenMount touch screen drivers support DOS, Windows 3.11, Windows 95, Windows 98, Windows Me, Windows NT, Windows 2000 and Linux operating systems under PC environment. The update drivers are available in our website, address is www.salt.com.tw, and users could download the new drivers from our home page.

TOUCH SCREEN

We offer a full range of touch screen sizes that excel in many applications and can be use with most flat panel LCD. The diagonally measured active area of our standard stock touch screens range from 3.8” to 20.1”.

When deciding on the right size of touch screen, keep in mind the following guidelines:

· Ensure the active area of the touch screen matches the active area of the display

· Ensure the viewing area of the touch screen is 0.76mm larger than the viewing area of the display.

· To mount the touch screen in the simplest way, ensure the display’s mounting hole is outside the perimeter of the touch screen.

· Review the latest specifications on our website.

Touch Screen Construction

Our touch screens are manufactured by Dynapro as a PL or FG construction. All constructions are scratch and chemical resistant, are sealable to NRMA 4X and provide reliable and accurate touch input, even when wearing gloves.

PL construction

Most customers use Dynarpo’s PL construction, which produces the most rugged analog resistive touch screen in the industry. The PL construction consists of two polyester layers bonded to a chemically strengthened in three to four times stronger than non-strengthened glass and a full optical lamination, Dynapro’s product provides added durability from breakage.
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FG construction

Customers who need superior touch screen optical quality in a less demanding environment prefer the FG construction. FG touch screens offer many of the same advantages as the PL construction touch screens but have fewer layers, resulting in greater transmission without break resistance. 
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TOUCH SCREE CONTROLLER

PenMount analog resistive controller is a device that works with the touch screen to decode the position of your touches. Our precise 1024-point resolution offers the high degree of control you need for accurate finger or stylus input.

PenMount touch screen solutions provides you with the level of support to best meet your manufacturing and design needs.  Our controllers are available in both serial and USB configurations, as a complete package, or a microcontroller chip.  The optional includes:

· Touch screen control board - contains the controller, cables for touch screen, power supply and serial port, this CD-Rom (drivers software) and stylus pen.

· Touch screen controller IC

PenMount 9584 control board and PenMount 9516 control board

The two boards function are same only difference in the mechanical size, picture is as below.

Both boards provides three cables, one is 4-wire or 8-wire cables for connecting to touch screen, the second cable is 2-wire power cable that is connected to 5V to 12N DC power, and the third cable is the 9-pin D-sub RS-232 cable
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PenMount 9512 controller IC

This controller is provided to the customer who layout to own board

No matter which type of controller you are using in the system, make sure that the right software drivers to install to your system.  

· For 9512 controller or PenMount 9584 and PenMount 9516 board, you have to use DMC9512 family drivers to install 

· For 9000 controller or PenMount 9084 board, you have to use DMC9000 family drivers to install

· For 5100 and 5600 controller or PenMount 5184 board, it is USB interface, you need to use DMC5100 family driver to install.

Each controller mark is stick on the top of CD-Rom, or you could read from all PenMount drivers easily.

TOUCH SCREE DRIVERS

PenMount drivers have different family, DMC9512, DMC9000 and DMC5100 family.  Please make sure the proper drivers to install.

For DMC9512 drivers

There are PenMount DOS, PenMount Windows 3.1, PenMount Windows 95/98/Me, PenMount Windows NT, PenMount Windows 2000 and Linux drivers available in this CD-Rom.  Please choose the right drivers for your system.  Other family drivers are also available in our website, address is http://www.salt.com.tw 

For any new version drivers, please visit our website for updated.
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