New Features in 4.40
XP Universal Driver 4.40 has the following new features:

· The XP Universal driver package has been localized to support the French, German, Spanish, Italian, Japanese, Simplified Chinese and Traditional Chinese.

· To keep the size of the Elo XP Universal driver default download package to a minimum,  the XP Universal Driver package is provided as two separate packages: 
  - Driver package

  - Users Guide

· The XP Universal Users Guide is also localized to support the French, German, Spanish, Italian, Japanese, Simplified Chinese and Traditional Chinese. The English Users Guide is included in the default download package. Language specific users guides can be downloaded from http://www.elotouch.com/Support/Downloads/default.asp
· Default calibration configuration values are saved in the Elo software registry key or in a file that can be modified to support user specific calibration values.
· Surface Capacitive calibration has been modified to automatically timeout after 30 seconds if there is no user interaction. Previous versions made five attempts before switching to the next monitor or exiting.

· The transparency of the right click on hold timeout icon is configured by a registry value entry. Please see Appendix A for details on how to use this feature.
· The initial delay before the right click on hold time out icon appears is configured by a registry value entry. Please see Appendix A for details on how to use this feature.

· If the system does not have a keyboard and mouse connected to it, the disable touch feature cannot be used from the task bar or control panel. 
· For Infrared touchmonitors, special support has been added to detect and report blocked beams. The Advanced page for the touchmonitor in the Control Panel is used to configure this feature. 
· A special hardware beep configuration feature for Infrared touchmonitors that include this special hardware feature has been added. The Advanced page for the touchmonitor in the Control Panel is used to configure this feature. 

· XPU 4.4 can be preinstalled on a system that has no support for a mouse or HID devices, however, this requires the user to insert the Windows system disk during the installation.
Bug fixed in this version:

· Intermittent loss of touch and activation of and the “Disable Touch” feature in the Elo control panel

· Windows Server 2003 would hang during the boot process because the Elo Service Application failed to load. 
· The EloGetTouch API function would not return touch data within a “no touch” rectangle. It now returns touch data irrespective of the touch rectangles defined on the screen.
· The EloGetTouch API function reports incorrect coordinates in ‘Drag’ mode. 
· The installation application sometimes causes a system message pop-up dialog box that prompts users to select the file location when installing a Serial only package. 

· The tool tray menu sometimes hides the taskbar. It now appears above the taskbar and is larger to permit easier option selection. 
· The touch mode sometimes changes to Mouse emulation mode after the video alignment application exited with a timeout. 
